1.

[Brand New](https://computerstore.lk/product/razer-thresher-7-1-pc-ps4-wireless-headset/)

**RAZER THRESHER 7.1 PC & PS4 WIRELESS HEADSET**

**LKR. 32,000**

* [**Description**](https://computerstore.lk/product/razer-thresher-7-1-pc-ps4-wireless-headset/#product-description)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| TECH SPECS |  |  |  |  |
|  |  |  |  |  |
| FREQUENCY RESPONSE | 12 – 28,000 Hz | |  |  |
|  |  |  |  |  |
| IMPEDANCE | 32Ω at 1kHz | |  |  |
|  |  |  |  |  |
| DRIVER SIZE – DIAMETERS (MM) | 50 mm |  |  |  |
|  |  |  |  |  |
| DRIVER TYPE | Neodymium Magnets | |  |  |
|  |  |  |  |  |
| See lessexpand\_less |  |  |  |  |
|  |  |  |  |  |
| EARPADS MATERIAL | Leatherette | |  |  |
|  |  |  |  |  |
| NOISE CANCELLING | Noise-isolating Leatherette Ear Cushions | | | |
|  |  |  |  |  |
| CONNECTION TYPE | RF 2.4GHz, up to 40ft / 12m | | |  |
|  |  |  |  |  |
| WEIGHT | 408g / 0.89lbs | |  |  |
|  |  |  |  |  |
| MICROPHONE STYLE | Retractable Uni-directional Boom Microphone | | | |
|  |  |  |  |  |
| VIRTUAL SURROUND ENCODING | Dolby® Headphone | |  |  |
|  |  |  |  |  |
| MICROPHONE FREQUENCY RESPONSE | 100 – 10,000 Hz | |  |  |
|  |  |  |  |  |
| VOLUME CONTROL | Volume & Mic Controls on headset | | | |
|  |  |  |  |  |
| OTHER CONTROLS | Volume & Mic Controls on headset | | | |
|  |  |  |  |  |
| BATTERY LIFE | Up to 16 hours on one single charge | | | |
|  |  |  |  |  |
| COMPATIBILITY | PlayStation 4 and PC | |  |  |
|  |  |  |  |  |
| MICROPHONE SENSITIVITY (@1KHZ) | -38 ± 3dB |  |  |  |

2.

[Brand New](https://computerstore.lk/product/razer-kraken-x-for-console-wired-console-gaming-headset/)

##### RAZER KRAKEN X FOR CONSOLE WIRED CONSOLE GAMING HEADSET

##### LKR. 16,000

* [**Description**](https://computerstore.lk/product/razer-kraken-x-for-console-wired-console-gaming-headset/#product-description)

**ULTRA-LIGHT COMFORT**

When gaming in the comfort of your own living room, you’ll want to feel relaxed so you can game on your console for hours on end. Enter the Razer Kraken X for Console. Ultra-light at just 250g with superior gaming audio. Sit tight and play for hours—your console gaming marathons are about to be a breeze.

**CLEAR & ACCURATE POSITIONAL AUDIO**

Featuring custom-tuned 40mm drivers, the Razer Kraken X produces clear and balanced sound from thundering explosions in all-out wars to subtle footsteps in stealthy covert operations.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  |  |  |  |  |
|  |  |  |  |  |
| TECH SPECS |  |  |  |  |
|  |  |  |  |  |
| FREQUENCY RESPONSE | 12 Hz – 28 kHz | |  |  |
|  |  |  |  |  |
| IMPEDANCE | 32 Ohm (1 kHz) | |  |  |
|  |  |  |  |  |
| SENSITIVITY | 109 dB (1 kHz) | |  |  |
|  |  |  |  |  |
| DRIVER SIZE – DIAMETERS (MM) | 40 mm |  |  |  |
|  |  |  |  |  |
| See lessexpand\_less |  |  |  |  |
|  |  |  |  |  |
| DRIVER TYPE | Custom Tuned | |  |  |
|  |  |  |  |  |
| EARCUPS | Oval Ear Cushions | |  |  |
|  |  |  |  |  |
| INNER EARCUP DIAMETER | Major Diameter 65 mm, Minor Diameter 44 mm | | | |
|  |  |  |  |  |
| EARPADS MATERIAL | Leatherette/ Foam | |  |  |
|  |  |  |  |  |
| NOISE CANCELLING | NA |  |  |  |
|  |  |  |  |  |
| CONNECTION TYPE | Analog 3.5 mm | |  |  |
|  |  |  |  |  |
| CABLE LENGTH | 1.3 m / 4.27 ft. | |  |  |
|  |  |  |  |  |
| WEIGHT | 250g / 0.55lbs | |  |  |
|  |  |  |  |  |
| MICROPHONE STYLE | Bendable cardioid microphone | | |  |
|  |  |  |  |  |
| PICK-UP PATTERN | Unidirectional ECM boom | | |  |
|  |  |  |  |  |
| VIRTUAL SURROUND ENCODING | NA |  |  |  |
|  |  |  |  |  |
| MICROPHONE FREQUENCY RESPONSE | 100 Hz – 10 kHz | |  |  |
|  |  |  |  |  |
| VOLUME CONTROL | On-earcup: Volume Up/Down | | |  |
|  |  |  |  |  |
| OTHER CONTROLS | On-earcup Mute Function: Click-to-mute | | | |
|  | On-earcup: Volume Up/Down | | |  |
|  |  |  |  |  |
| BATTERY LIFE | NA |  |  |  |
|  |  |  |  |  |
| LIGHTING | NA |  |  |  |
|  |  |  |  |  |
| COMPATIBILITY | Cross-Platform | |  |  |
|  |  |  |  |  |
| MICROPHONE SENSITIVITY (@1KHZ) | -45 ± 3 dB | |  |  |

3.

[Brand New](https://computerstore.lk/product/razer-hammerhead-true-wireless-earbuds-black-true-wireless-earbuds/)

##### RAZER HAMMERHEAD TRUE WIRELESS EARBUDS – BLACK TRUE WIRELESS EARBUDS

##### LKR. 30,500

* [**Description**](https://computerstore.lk/product/razer-hammerhead-true-wireless-earbuds-black-true-wireless-earbuds/#product-description)

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| TECH SPECS |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| HEADPHONE FREQUENCY RESPONSE | 20 Hz – 20 KHz | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| HEADPHONE IMPEDANCE | 32 Ohm (1 kHz) | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| HEADPHONE SENSITIVITY | 91 ± 3 dB (1 kHz) | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| HEADPHONE INPUT POWER | 8 mW |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| HEADPHONE DRIVERS | 13 mm |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| HEADPHONE CONNECTOR | Bluetooth |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| CABLE LENGTH | None |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| WEIGHT | 45 g |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| MICROPHONE PICK UP PATTERN | Omnidirectional | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| MICROPHONE SIGNAL-TO-NOISE RATIO | ≥ 55 dB |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| MICROPHONE SENSITIVITY (@1KHZ) | 42 ± 3 dB (1 kHz) | |  |  |  |  |  |
|  |  |  |  |  |  |  |  |
| COMPATIBILITY | Devices with Bluetooth connections | | | |  |  |  |
|  | Smartphone app available for Android™ 8.0 Oreo and iOS 11 (or higher) | | | | | | |

4.

[Brand New](https://computerstore.lk/product/razer-hammerhead-duo-compatible-with-the-nintendo-switch-dual-driver-in-ears/)

##### RAZER HAMMERHEAD DUO – COMPATIBLE WITH THE NINTENDO SWITCH™ DUAL DRIVER IN-EARS

##### LKR. 18,000

* [**Description**](https://computerstore.lk/product/razer-hammerhead-duo-compatible-with-the-nintendo-switch-dual-driver-in-ears/#product-description)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| TECH SPECS |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| HEADPHONE FREQUENCY RESPONSE | 20 Hz-20 KHz | |  |  |  |  |
|  |  |  |  |  |  |  |
| HEADPHONE IMPEDANCE | 32 Ω ± 15% | |  |  |  |  |
|  |  |  |  |  |  |  |
| HEADPHONE SENSITIVITY | 112 ± 3 dB (Max SPL) | | |  |  |  |
|  |  |  |  |  |  |  |
| HEADPHONE INPUT POWER | 10 mW / 20 mW | |  |  |  |  |
|  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| HEADPHONE DRIVERS | Dynamic + Balanced Armature | | |  |  |  |
|  |  |  |  |  |  |  |
| HEADPHONE CONNECTOR | 3.5 mm angled jack | |  |  |  |  |
|  |  |  |  |  |  |  |
| CABLE LENGTH | 1.2 m |  |  |  |  |  |
|  |  |  |  |  |  |  |
| WEIGHT | 17 g |  |  |  |  |  |
|  |  |  |  |  |  |  |
| MICROPHONE FREQUENCY RESPONSE | 100 Hz -10 kHz | |  |  |  |  |
|  |  |  |  |  |  |  |
| MICROPHONE PICK UP PATTERN | Omni-directional | |  |  |  |  |
|  |  |  |  |  |  |  |
| MICROPHONE SIGNAL-TO-NOISE RATIO | ≥ 58 dB |  |  |  |  |  |
|  |  |  |  |  |  |  |
| MICROPHONE SENSITIVITY (@1KHZ) | -40 ± 3 dB | |  |  |  |  |
|  |  |  |  |  |  |  |
| COMPATIBILITY | Devices with 3.5 mm audio jack | | |  |  |  |
|  | Devices with 3.5 mm audio + microphone combined jack | | | | | |

5.

##### RAZER BLACKSHARK V2 X MULTI-PLATFORM WIRED ESPORTS HEADSET

##### LKR. 19,500

* [**Description**](https://computerstore.lk/product/razer-blackshark-v2-x-multi-platform-wired-esports-headset/#product-description)
* THE SOUND OF ESPORTS
* Face the competition head-on with a lightweight esports headset that thrives under pressure. Introducing the Razer BlackShark V2 X—a triple threat of amazing audio, superior mic clarity and supreme sound isolation that’s approved by pros.
* RAZER™ HYPERCLEAR CARDIOID MIC
* Offering greater speech pickup and noise cancellation, the bendable mic on this lightweight esports headset has an optimized microphone housing which adopts a more open design for minimal obstruction—resulting in improved clarity for a closer recreation of your voice
* ADVANCED PASSIVE NOISE CANCELLATION
* From cheering crowds to the hum of your rig, shut noise out and enjoy uninterrupted focus with special closed earcups that fully cover your ears, aided by plush cushions that form a closer seal for greater sound isolation.
* LIGHTWEIGHT COMFORT
* At just 240g, you’ll barely remember you have it on during gaming marathons. The headset is made even more comfortable thanks to thicker heading padding and improved memory foam ear cushions wrapped in a combination of breathable fabric and plush leatherette.
* 7.1 SURROUND SOUND
* Heighten your match awareness and let nothing escape your ears with accurate positional audio that lets you pinpoint intuitively where every sound is coming from.
* \*Only available on Windows 10 64bit
* CROSS-PLATFORM COMPATIBILITY
* This lightweight esports headset uses a 3.5mm jack and works across popular platforms, allowing you to seek out competition on PC, Mac, PS4, Xbox One, Nintendo Switch and mobile devices\*.
* \*Mobile devices with an available 3.5mm port

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| TECH SPECS |  |  |  |  |  |  |
|  |  |  |  |  |  |  |
| FREQUENCY RESPONSE | 12 Hz – 28 kHz | |  |  |  |  |
|  |  |  |  |  |  |  |
| IMPEDANCE | 32 Ω (1 kHz) | |  |  |  |  |
|  |  |  |  |  |  |  |
| SENSITIVITY | 100 dBSPL/mW, 1 kHz | | |  |  |  |
|  |  |  |  |  |  |  |
| DRIVER SIZE – DIAMETERS (MM) | 50 mm |  |  |  |  |  |
|  |  |  |  |  |  |  |
| DRIVER TYPE | Razer™ TriForce | |  |  |  |  |
|  |  |  |  |  |  |  |
| EARCUPS | Breathable memory foam cushions | | | |  |  |
|  |  |  |  |  |  |  |
| INNER EARCUP DIAMETER | 2.48″ x 1.69″ | |  |  |  |  |
|  | 63 mm x 43 mm | |  |  |  |  |
|  |  |  |  |  |  |  |
| EARPADS MATERIAL | Breathable memory foam | | |  |  |  |
|  |  |  |  |  |  |  |
| NOISE CANCELLING | Advanced passive noise cancellation | | | |  |  |
|  |  |  |  |  |  |  |
| CONNECTION TYPE | Analog 3.5 mm | |  |  |  |  |
|  |  |  |  |  |  |  |
| CABLE LENGTH | 1.3 m / 4.27 ft. | |  |  |  |  |
|  |  |  |  |  |  |  |
| WEIGHT | 0.53 lbs / 240 g | |  |  |  |  |
|  |  |  |  |  |  |  |
| MICROPHONE STYLE | Razer™ HyperClear Cardioid Mic | | |  |  |  |
|  |  |  |  |  |  |  |
| PICK-UP PATTERN | Unidirectional | |  |  |  |  |
|  |  |  |  |  |  |  |
| MICROPHONE FREQUENCY RESPONSE | 100 Hz – 10 kHz | |  |  |  |  |
|  |  |  |  |  |  |  |
| MICROPHONE SENSITIVITY (@1KHZ) | -42 dB V/Pa, 1 kHz | |  |  |  |  |
|  |  |  |  |  |  |  |
| VIRTUAL SURROUND ENCODING | 7.1 Surround Sound\* | |  |  |  |  |
|  | \*Only available on Windows 10 64-bit | | | |  |  |
|  |  |  |  |  |  |  |
| VOLUME CONTROL | On-earcup: Volume Up/ Down | | |  |  |  |
|  |  |  |  |  |  |  |
| OTHER CONTROLS | On-earcup controls – Mic mute on/off toggle | | | |  |  |
|  |  |  |  |  |  |  |
| BATTERY LIFE | NA |  |  |  |  |  |
|  |  |  |  |  |  |  |
| LIGHTING | NA |  |  |  |  |  |
|  |  |  |  |  |  |  |
| COMPATIBILITY | PC, Mac, PS4, Xbox One, Nintendo Switch and mobile devices\* | | | | | |
|  | \*Mobile devices with an available 3.5mm port | | | | |  |



6.

##### MSI DS502 GAMING HEADSET

##### LKR. 11,500

7.

[Brand New](https://computerstore.lk/product/msi-ds501-3-5mm-connector-circumaural-gaming-headset/)

##### MSI DS501 3.5MM CONNECTOR CIRCUMAURAL GAMING HEADSET

##### LKR. 7,500

8.

##### Jedel V2000 (GH-39) Headset 7.1 Channel 3.5mm GAMING HEADSET

##### LKR. 2,850

|  |  |
| --- | --- |
| onnectivity Technology | Wired |
| Brand | Paialu |
| Material | Leather, Plastic, Metal |
| Headphones Jack | 3.5 millimeters |
| Item Weight | 0.4 Pounds |

9.

##### HYPERX CLOUD STINGER S 7.1 SURROUNDING SOUND GAMING HEADSET

##### LKR. 19,000

|  |  |  |
| --- | --- | --- |
| Specifications |  |  |
|  |  |  |
| Headphone |  |  |
|  |  |  |
| Driver |  | Dynamic, 50mm with neodymium magnets |
|  |  |  |
| Type |  | Circumaural, Closed back |
|  |  |  |
| Frequency response |  | 18Hz-23kHz |
|  |  |  |
| Impedance |  | 32 Ω |
|  |  |  |
| Sound pressure level |  | 95.5dBSPL/mW at 1kHz |
|  |  |  |
| T.H.D. |  | ≤ 2% |
|  |  |  |
| Weight |  | 275g |
|  |  |  |
| Cable length |  | 2.5m |
|  |  |  |
| Connection type |  | 3.5mm plug (4 pole) |
|  |  |  |
| Microphone |  |  |
|  |  |  |
| Element |  | Electret condenser microphone |
|  |  |  |
| Polar pattern |  | Uni-directional, Noise-cancelling |
|  |  |  |
| Frequency response |  | 50Hz-18kHz |
|  |  |  |
| Sensitivity |  | -40dBV (1V/Pa at 1kHz) |
|  |  |  |
| USB Adapter |  |  |
|  |  |  |
| Weight |  | 12g |
|  |  |  |
| Cable length |  | 0.15m |

10

[Brand New](https://computerstore.lk/product/gamdias-hebe-e3-rgb-surrounding-sound-usb-gaming-headset/)

##### GAMDIAS HEBE E3 RGB SURROUNDING SOUND USB GAMING HEADSET

##### LKR. 7,000

|  |  |  |
| --- | --- | --- |
| Specifications |  |  |
|  |  |  |
| Sensitivity |  | 110±3dB |
| Impedance |  | 64 Ohm + / ​​- 15% |
| Driver diameter |  | 53mm |
| Driver Magnet |  | NdFeB |
| Microphone size |  | Φ6\*2.7mm |
| Microphone Sensitivity |  | -42db±3db |
| Microphone Pick up Pattern |  | Omnidirectional |
| Cable Length |  | 2m |
| Plug type |  | USB |
| Dimension (LxWxH) |  | 170 x 105 x 225 |
| Application UI |  | Yes |

Top of Form

Bottom of Form