1.

[Brand New](https://computerstore.lk/product/raidmax-x616-mid-tower-gaming-case/)

**RAIDMAX X616 MID-TOWER GAMING CASE**

**LKR. 14,000**

Description

» PART NUMBER:X616

» CASE TYPE:ATX – Mid Tower

» SIDE PANEL:Tempered Glass

» LIGHTING:RGB

» STOCK AVAILABILITY:In stock

2.

##### CORSAIR ICUE 5000X RGB TEMPERED GLASS MID-TOWER ATX PC SMART CASE – BLACK

##### LKR. 51,500

|  |  |  |
| --- | --- | --- |
| Case Dimensions |  | 520mm x 245mm x 520mm |
|  |  |  |
|  |  |  |
| Maximum GPU Length |  | 400 |
|  |  |  |
|  |  |  |
| Maximum PSU Length |  | 250 |
|  |  |  |
|  |  |  |
| Maximum CPU Cooler Height |  | 170 |
|  |  |  |
|  |  |  |
| Expansion Slots |  | 7 vertical + 2 horizontal |
|  |  |  |
|  |  |  |
| Case Drive Bays |  | (x2) 3.5in (x4) 2.5in |
|  |  |  |
|  |  |  |
| Form Factor |  | NA |
|  |  |  |
|  |  |  |
| Case Windowed |  | Tempered Glass |
|  |  |  |
|  |  |  |
| Corsair Link Enabled |  | Yes |
|  |  |  |
|  |  |  |
| Color |  | BLACK |
|  |  |  |
|  |  |  |
| Case Material |  | Steel, Tempered Glass, Plastic |
|  |  |  |
|  |  |  |
| Radiator Compatibility |  | 120mm, 140mm, 240mm, 280mm, 360mm |
|  |  |  |
|  |  |  |
| Case Front IO |  | (1x) USB 3.1 Type C, (2x) USB 3.0, (1x) Audio in/out |
|  |  |  |
|  |  |  |
| Compatible Corsair Liquid Coolers |  | H55, H60, H75, H80i, H90, H100i, H105, H110i, H115i, H150i |
|  |  |  |
|  |  |  |
| Case Power Supply |  | ATX |
|  |  |  |
|  |  |  |
| Weight |  | 13.84 |

3. [Brand New](https://computerstore.lk/product/corsair-icue-4000x-rgb-tempered-glass-mid-tower-atx-case-black/)

**CORSAIR ICUE 4000X RGB TEMPERED GLASS MID-TOWER ATX CASE – BLACK**

**LKR. 34,500**

|  |  |  |
| --- | --- | --- |
| Case Dimensions |  | 453mm x 230mm x 466mm |
|  |  |  |
|  |  |  |
| Maximum GPU Length |  | 360mm |
|  |  |  |
|  |  |  |
| Maximum PSU Length |  | 180mm (220mm if HDD cage removed) |
|  |  |  |
|  |  |  |
| Maximum CPU Cooler Height |  | 170mm |
|  |  |  |
|  |  |  |
| Expansion Slots |  | 7+2 vertical |
|  |  |  |
|  |  |  |
| Case Drive Bays |  | (x2) 3.5in (x2) 2.5in |
|  |  |  |
|  |  |  |
| Form Factor |  | Mid-Tower |
|  |  |  |
|  |  |  |
| Case Windowed |  | Tempered Glass |
|  |  |  |
|  |  |  |
| Corsair Link Enabled |  | Yes |
|  |  |  |
|  |  |  |
| Color |  | Black |
|  |  |  |
|  |  |  |
| Case Material |  | Steel, Tempered Glass, Plastic |
|  |  |  |
|  |  |  |
| Radiator Compatibility |  | 120mm, 140mm, 240mm, 280mm, 360mm |
|  |  |  |
|  |  |  |
| Compatible Corsair Liquid Coolers |  | H55, H60, H75, H80i, H90, H100i, H105, H110i, H115i, H150i |
|  |  |  |
|  |  |  |
| Case Power Supply |  | ATX (not included) |
|  |  |  |
|  |  |  |
| Weight |  | 7.8kg/17.20lbs |
|  |  |  |
|  |  |  |
| Lighting |  | RGB |
|  |  |  |
|  |  |  |
| Drive Bays 3.5″ |  | 2 |
|  |  |  |
|  |  |  |
| Drive Bays 2.5″ |  | 2 |

4.

[Used](https://computerstore.lk/product/corsair-graphite-series-780t-full-tower-black-pc-case/)

**CORSAIR GRAPHITE SERIES 780T FULL-TOWER BLACK PC CASE**

**LKR. 45,000**

» BRAND:  
Corsair  
» PART NUMBER:  
CC-9011063-WW  
» CASE TYPE:  
ATX – Full Tower  
» SIDE PANEL:  
Glass Windowed  
» LIGHTING:  
Single Color  
» STOCK AVAILABILITY:  
In stock  
DESCRIPTION :  
Case Dimensions

5.

[Brand New](https://computerstore.lk/product/nzxt-h710-mid-tower-white-and-black-case/)

**NZXT H710 MID TOWER WHITE AND BLACK CASE**

**LKR. 31,500**

**Availability: In Stock**

##### Specifications

* **PART NUMBER:CA** - H710B-W1
* **CASE TYPE:ATX**- Full Tower
* **SIDE PANEL:Tempered Glass**

Description

|  |  |
| --- | --- |
| Dimensions | W: 230mm H: 516mm D: 494mm (with feet) |
|  |  |
| Material(s) | SGCC Steel and Tempered Glass |
|  |  |
| Weight | 12.1 kg |
|  |  |
| Motherboard Support | Mini-ITX, MicroATX, ATX and EATX (Up to 272mm or 10.7-inches) |
|  |  |
| Front I/O Ports | 1x USB 3.1 Gen 2 Type-C |
|  | 2x USB 3.1 Gen 1 Type-A |
|  | 1x Headset Audio Jack |
|  | Front I/O internal header |
|  | 1x USB 3.1 Gen 2 Internal Header |
|  | 1x USB 3.1 Gen 1 Internal Header |
|  | 1x HD Audio Header |
|  |  |
| Filters | All Air Intakes |
|  |  |
| Included Accessories | Installation screws |
|  | 10x Cable ties |
|  | 1x Headset Audio Jack Splitter (4 pole to 3 pole) |
|  |  |
| Expansion Slots | 7 |
|  |  |
| Drive Bays | 2.5”: 7 |
|  | 3.5”: 2+2 |
|  |  |
| Radiator Support | Front: 2x 140 or 3x 120mm with Push/Pull |
|  | Top: 2x 140 or 3x 120 |
|  | Rear: 1x 120 |
|  |  |
| Fan Support | Front: 3x 120/ 2x 140mm (3 Aer F120 Case Version included) |
|  | Top: 3x 120/2x 140mm |
|  | Rear: 1x 120/1x 140mm (1 Aer F140 Case Version included) |
|  |  |
| Fan Specs | Aer F120 (Case Version) |
|  | Speed: 1200 ± 200 RPM |
|  | Airflow: 50.42 |
|  | CFM Noise: 28 dBA |
|  | Bearing: Rifle Bearing |
|  | Aer F140 (Case Version) |
|  | Speed: 1,000 ± 200 RPM |
|  | Airflow: 68.95 CFM |
|  | Noise: 29 dBA |
|  | Bearing: Rifle Bearing |
|  |  |
| Clearance | Cable Management: 18-22mm |
|  | GPU Clearance: Up to 413mm |
|  | CPU Cooler: Up to 185mm |
|  | Front Radiator: 60mm |
|  | Top Radiator: 30mm |
|  | Reservoir & Pump: Up to 224mm (Along cable bar) |
|  |  |
| Compatibility | NVIDIA GeForce RTX 30 series case compatibility chart |
|  |  |
| Warranty | 2 Years |
|  |  |
| Model Number | CA-H710B-W1 |
|  |  |
| EAN | 5.0603E+12 |
|  |  |
| UPC | 8.15671E+11 |

6.

[Brand New](https://computerstore.lk/product/corsair-110r-tempered-glass-mid-tower-atx-case-2/)

**CORSAIR 110R TEMPERED GLASS MID-TOWER ATX CASE**

**LKR. 15,000**

**Availability: In Stock**

Specifications

* **PART NUMBER:CC** - 9011183-WW
* **CASE TYPE:ATX**- Mid Tower
* **SIDE PANEL:Tempered Glass**
* [**Description**](https://computerstore.lk/product/corsair-110r-tempered-glass-mid-tower-atx-case-2/#product-description)

|  |  |
| --- | --- |
| ase Dimensions | 418mm x 210mm x 480mm |
| Maximum GPU Length | 330mm |
| Maximum PSU Length | 180mm |
| Maximum CPU Cooler Height | 160mm |
| Case Expansion Slots | 7 |
| Case Drive Bays | ”(x2) 3.5in (x2) 2.5in” |
| Case Form Factor | Mid-Tower |
| Case Windowed | Tempered Glass |
| iCUE enabled | No |
| Case Material | Steel, Tempered Glass |
| Radiator Compatibility | 120mm, 140mm, 240mm, 280mm |
| Compatible Corsair Liquid Coolers | H55, H60, H75, H80i, H90, H100i, H105, H110i, H115i |
| Case Power Supply | ATX (not included) |
| Weight | 6.5kg / 14.2lbs |
| Case Drive Bays 3.5″ | 2 |
| Case Drive Bays 2.5″ | 2 |

7

[Brand New](https://computerstore.lk/product/raidmax-e105-rgb-micro-atx-case/)

##### RAIDMAX E105 RGB MICRO ATX CASE

##### LKR. 6,500

Specifications

* **BRAND:Raidmax**
* **PART NUMBER:Raidmax E105 RGB**
* **CASE TYPE:ATX**- Mid Tower
* [**Description**](https://computerstore.lk/product/raidmax-e105-rgb-micro-atx-case/#product-description)

|  |  |  |
| --- | --- | --- |
| Model Number |  | E105 |
|  |  |  |
| Material |  | SPCC 0.4mm, Black interior |
|  |  |  |
| Case Size |  | L330xW180xH410 mm |
|  |  |  |
| Cartoon Size |  | L450xW225xH440 mm |
|  |  |  |
| Mother Board Support |  | ATX/ M-ATX/ ITX |
|  |  |  |
| Drive Bays |  | 5.25″EXT x2 / 3.5″HDD x2 / 2.5″SSD x2 |
|  |  |  |
| PCI Slots |  | 7 Slots |
|  |  |  |
| I/O Panel |  | USB 2.0 x2; HD Audio x1 |
|  |  |  |
| Cooling System |  | Front : 1x 120mm fan (included) |
|  |  | Rear : 1x 120mm fan (included) |
|  |  |  |
| Max CPU Cooler height |  | 160 mm |
|  |  |  |
| Max VGA Card Length |  | 320 mm |

8.

[Brand New](https://computerstore.lk/product/nzxt-h510-compact-mid-tower-white-and-black-case-2/)

##### NZXT H510 COMPACT MID TOWER WHITE AND BLACK CASE

##### LKR. 17,500

* [**Specifications**](https://computerstore.lk/product/nzxt-h510-compact-mid-tower-white-and-black-case-2/#product-specifications)
* **BRAND:NZXT**
* **PART NUMBER:CA** - H510B-W1
* **CASE TYPE:ATX**- Mid Tower
* **SIDE PANEL:Tempered Glass**
* [**Description**](https://computerstore.lk/product/nzxt-h510-compact-mid-tower-white-and-black-case-2/#product-description)

|  |  |
| --- | --- |
| Dimensions | W: 210mm H: 435mm D: 428mm (without feet) |
|  | W: 210mm H: 460mm D: 428mm (with feet) |
| Material(s) | SGCC Steel, Tempered Glass |
| Weight | 6.6 kg |
| Motherboard Support | Mini-ITX, MicroATX, and ATX |
| Front I/O Ports | H510: |
|  | 1x USB 3.1 Gen 2 Type-C |
|  | 1x USB 3.1 Gen 1 Type-A |
|  | 1x Headset audio Jack |
|  | H511 (\*SI only): |
|  | 2x USB 3.1 Gen 1 Type-A |
|  | 1x Headset audio Jack |
|  |  |
|  | Front I/O internal header |
|  | 1x USB 3.1 Gen 2 Internal Header |
|  | 1x USB 3.1 Gen 1 Internal Header |
|  | 1x HD Audio Header |
| Filters | All Air Intakes |
| Included Accessories | Installation screws |
|  | 10x Cable ties |
|  | 1x Headset Audio Jack splitter (4 pole to 3 pole) |
| Drive Bays | 2.5”: 2+1 |
|  | 3.5”: 2+1 |
| Expansion Slots | 7 |
| Radiator Support | Front: 2x 140 or 2x 120mm with Pull |
|  | Rear: 1x 120mm |
| UPC | 815671014764 |
| Fan Support | Front: 2 x 120/ 2 x 140mm |
|  | Top: 1x 120mm/ 1x 140mm (1 Aer F120 Case Version included) |
|  | Rear: 1x 120mm (1 Aer F120 Case Version included) |
| Fan Specs | Aer F120 (Case Version) |
|  | Speed: 1200 ± 200 RPM |
|  | Airflow: 50.42 CFM |
|  | Noise: 28 dBA |
|  | Bearing: Rifle Bearing |
| Clearance | Cable Management: 19-23mm |
|  | GPU Clearance: Up to 381mm w/o front watercooler installed, up to 325mm with front watercooler installed |
|  | CPU Cooler: Up to 165mm |
|  | Front Radiator: 60mm |
|  | Rear Radiator: 60mm |
|  | Reservoir & Pump: Up to 180mm (Along cable bar), Up to 86mm (Along bottom panel) |
|  |  |
| Model Number | CA-H510B-W1 |
| EAN | 5060301695065 |

9.

[Brand New](https://computerstore.lk/product/raidmax-exo-blue-micro-atx-case/)

##### Raidmax exo blue micro atx case

##### LKR. 6,500

##### Specifications

* **MODEL NAME – EXO**
* **AVAILABLE COLOR – BLUE/GREEN/ RED**
* **DIMENTIONS – 427[L] \* 195 [W] \* 420 [H] mm**
* **EXTERNAL DRIVE BAYS – 5.25’’ \*2**
* **INTERNAL DRIVE BAYS – 2.5” SSD \* 2, 3.5” H.D \*4**
* **SYSTEM BOARD**- Micro ATX / ATX
* **EXPANSION SLOTS – 7 slots**
* **I / O PORTS – 1\* USB2.0, 1\*USB3.0, 2\*HD Audio**
* **SUPPORT – 150mm high CPU cooler / 355mm VGA card / 120mm**- 360mm liquid cooling
* **COOLING SYSTEM**
* **FRONT – 120mm \* 2 [one 120mm LED fan included]**
* **SIDE – None**
* **BACK – 80mm\*1**
* **TOP – None**
* **BOTTOM**- None
* [**Description**](https://computerstore.lk/product/raidmax-exo-blue-micro-atx-case/#product-description)

10

[Brand New](https://computerstore.lk/product/raidmax-galaxy-micro-atx-case/)

##### Raidmax galaxy micro atx case

##### LKR. 9,000

##### Specifications

* **MODEL NAME – Galaxy (G23)**
* **AVAILABLE COLOR – Black**
* **DIMENTIONS – 423.6\*191\*408mm**
* **EXTERNAL DRIVE BAYS – none**
* **INTERNAL DRIVE BAYS – 2.5” H.D \* 3, 3.5” H.D \*2**
* **SYSTEM BOARD**- Mini-ITX / Micro-ATX / ATX
* **EXPANSION SLOTS – 7 slots**
* **I / O PORTS –USB3.0, 1 / USB2.0\* 1 / HD Audio \*2**
* **SUPPORT – 14mm high CPU cooler / 355mm VGA card**
* **COOLING SYSTEM**
* **FRONT – None**
* **SIDE – None**
* **BACK – 80mm\*1**
* **TOP – None**
* **BOTTOM**- None